| A picture containing text, clipart  Description automatically generated  ADULT FAMILY HOME (AFH)  **AFH Initial Licensing Inspection: Resident Bedroom/Bathroom Worksheet Continuation** | | | APPLICANT’S / ER’S NAME | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| APPLICANT CONTACT PHONE NUMBER | | | AFH SITE PHONE NUMBER | | |
| AFH NAME | | | | | |
| AFH SITE ADDRESS | | EMAIL ADDRESS | | | | | | |
| DISTRICT / UNIT | | | COUNTY | | INSPECTION TYPE  **Initial** | 12 MONTH DATE |
| FIELD MANAGER’S NAME | | FM PHONE | | | | | LICENSOR’S NAME | |
|  | | | | | | | | |
| **Bedroom** Measurements: Length (L) x Width (W) divided by 144 = Square Feet (Sq. Ft.) | | | | | | | | |
| Evacuation Level  I  I/ A | Subtotal Sq. Ft. = | | |  | | | | |
| - Closet / Storage | | |
| - Door Swing | | |
| Capacity  1  2 | - Other | | |
| - Other | | |
| **= Usable Sq. Ft.** | | |
| **\*M N N/A**  **Exit does not pass through another room:**  **\*M N N/A**  **Window:\*\***    Door opening device  Unobstructed    **Clean:**  Windowsill height does not exceed 44”    **Closet / Storage:**  Screens    Open-able  Privacy    Floor Guides  Open-able    **Heat Source:**  **Lighting:**  **Door:**  Lock  Doorway width minimum 27 inches | | | | **\*\* Window specifications: Minimum height – 24”, Minimum width – 20”, Minimum square footage opening – 5.7 sq.ft. except at grade level where it may be 5 sq.ft.** | | | | |
| **Bathroom attached to Bedroom \*M N N/A \*M N N/A**  **Accessibility Level:**  I  I/ A    **General:**  **Door:**    Sanitation  Lock with opening device    Toxics inaccessible  Unobstructed    TP holder  Doorway width minimum 27 inches    Toilet grab bars secure  **Shower / Tub:**    Window cover / screens  Shower / tub grab bars secure    Lighting   Non-Skid Surface    Other | | | |  | | | | |